Spalart-Allmaras model

Solve for transport with model equation for the RHS.

Prescribe the value for at the inlet according to where is the mean flow velocity, is turbulence intensity (usually 5%) and turbulent length scale. For external flows, take turbulent length scale to be the momentum thickness. For internal flows where is the hydraulic diameter.

and models